[Prev][Next][Index][Thread]

# Re: USR1 signal

- Date: Wed, 27 Sep 1995 09:54:25 PDT
- From:
- Cc: moo-cows@parc.xerox.com
- In-reply-to: Thomas Wouters's message of "Wed, 27 Sep 1995 05:21:12 PDT" <Pine.SOL.3.91.950927125931.474J-100000@alibaba.dds.nl>

    Thomas Wouters writes:
    > Now if the MOO wouldn't shutdown, we could try and figure out where the
    > problem lies -- in the system, the scsi-interface (swap memory), the
    > physical memory, or the MOO...

    I would suggest attaching a debugger to the MOO process with a breakpoint in
    the function `panic()'.  When it stops, you can look up the stack to see where
    the problem is coming from.

    	Pavel

References:

- USR1 signal

- From: Thomas Wouters <zonny@alibaba.dds.nl>

- Prev: USR1 signal
- Next: VEIL Protocol
- Index: MOO-cows
- Thread: MOO-cows

Home | Subject Index | Thread Index