# Server limitations on network I/O

Michael Brundage (brundage@laurel.ipac.caltech.edu)
Sat, 19 Jul 1997 16:47:31 -0700 (PDT)

- Messages sorted by:[ date ][ thread ][ subject ][ author ]

    Couple o' questions:

    (1) What is the range of ASCII values which the server will accept (or
    output) through non-binary I/O?

    (2) What is the maximum line length, both incoming and outgoing?

    Are the answers platform-specific?  For modified MOO's (such as those
    handling Japanese), are the answers different than for the stock MOO server?

    Thanks,

    michael
    brundage@ipac.caltech.edu