[Subject Prev][Subject Next][Thread Prev][Thread Next][Subject Index][Thread Index]

# Server limitations on network I/O

- Date: Sat, 19 Jul 1997 16:47:31 -0700 (PDT)
- From:
- Content-Type: TEXT/PLAIN; charset=US-ASCII

    Couple o' questions:

    (1) What is the range of ASCII values which the server will accept (or
    output) through non-binary I/O?

    (2) What is the maximum line length, both incoming and outgoing?

    Are the answers platform-specific?  For modified MOO's (such as those
    handling Japanese), are the answers different than for the stock MOO server?

    Thanks,

    michael
    brundage@ipac.caltech.edu

Follow-Ups:

- Re: Server limitations on network I/O

- From: Andreas Bogk <andreas@artcom.de>

- Prev by Subject: Request for help, MacGoesMOO
- Next by Subject: Re: Server limitations on network I/O
- Prev by thread: Debugging Room released
- Next by thread: Re: Server limitations on network I/O
- Index(es):
  - Subject
  - Thread

Home | Subject Index | Thread Index